**DTBC 2200**

**Coil Cleaner**

**DTBC 2200**

**Blank Cleaner**

[**1.** **GENERAL DESCRIPTION** 2](#_Toc124348799)

[**1.1** **CUSTOMER TECHNICAL DATA** 3](#_Toc124348800)

[**1.2** **MACHINES TECHNICAL DATA** 4](#_Toc124348801)

[**2.** **MAIN HOUSING** 5](#_Toc124348802)

[**3.** **GENERAL DESCRIPTION COIL BRUSH CLEANER** 7](#_Toc124348803)

[**4.** **GENERAL DESCRIPTION BLANKS BRUSH CLEANER** 9](#_Toc124348804)

[**5.** **GENERAL SPECIFICATIONS INCLUDING IN THE QUOTE** 11](#_Toc124348805)

# **GENERAL DESCRIPTION**

The scope of supply for this quotation consists in the detailed design, procurement, fabrication and assembly of auxiliary elements related to the below description of material and in-house testing.

The machine is suitable for the installation on a blanking line.

The proposal is composed from:

Brush Cleaner for the coil

Brush Cleaner for blanks on the stacker

While running through the cleaner, the coil is cleaned on both sides by linear brushes. The dirt is stripped out from the brushes transported into a filter by suction system. These results are possible thanks to:

- mechanical brush effect by the linear brush

- capillary adhesive forces between micro- moistened filament and particle

- reduction of electrostatic charges brought about by the DTBR\_300 (Ingromat) liquid.

# **CUSTOMER TECHNICAL DATA**

|  |  |
| --- | --- |
| DTBC 2200 Coil Cleaner |  |
| Type of materials | Steel, Aluminum |
| Thickness | 0,5 – 3 mm |
| Material width (left to right) | Min 400 max 2200 mm |
| Material shape | Coil |
| Working speed | Max 110 m/min |
| Total installed power supply brush cleaner | 8 kW |
| Electrical equipment | 380V, 50 Hz, 3 phases, N, PE (different voltage available) |
| Safety interface | Safety PLC |
| Labelling | Standard Dietronic |
| Application | Coil |
|  |  |

|  |  |
| --- | --- |
| DTBC 2200 Blank Cleaner |  |
| Type of materials | Steel, Aluminum |
| Thickness | 0,5 – 3 mm |
| Max Thickness delta | 2 mm |
| Material width (left to right) | Min 400 max 3800 mm |
| Material length (front to back) | Min 400 max 3800 mm |
| Material shape | Blanks - rectangle, trapezoid, parallelogram, any shape |
| Working speed | Max 200 m/min |
| Total installed power supply brush cleaner | 6 kW |
| Electrical equipment | 380V, 50 Hz, 3 phases, N, PE (different voltage available) |
| Safety interface | Safety PLC |
| Labelling | Standard Dietronic |
| Application | Blanks |
|  |  |

# **MACHINES TECHNICAL DATA**

|  |  |
| --- | --- |
| **DTBC 2200 Coil Cleaner** |  |
| **Total installed power supply brush cleaner** | 8 kW |
| **Electrical equipment** | 380V, 50 Hz, 3 phases, N, PE (different voltage available) |
| **General valve voltage** | 24 V DC |
| **Control voltage** | 24 V DC |
| **Coil brush cleaner air consumption** | 1200 Nl/min at 6 bar |
| **Air Supply (brush cleaner)** | 5 bar min |
| **Communication with a line** | Profinet |
| **Safety interface** | Safety PLC |

|  |  |
| --- | --- |
| **DTBC 2200 Blank Cleaner** |  |
| **Total installed power supply brush cleaner** | 6 kW |
| **Electrical equipment** | 380V, 50 Hz, 3 phases, N, PE (different voltage available) |
| **General valve voltage** | 24 V DC |
| **Control voltage** | 24 V DC |
| **Blank brush cleaner air consumption** | 1200 Nl/min at 6 bar |
| **Air Supply (brush cleaner)** | 5 bar min |
| **Communication with a line** | Profinet |
| **Safety interface** | Safety PLC |

# **MAIN HOUSING**

**Frame**

The machine’s substructure is a solid and waterproof welded steel construction.

**Interface points with a press line for both machines**

The electrics and pneumatics connections pass along the machine side in a cable chain and can be plugged at both sides a separate connection box for the Cleaner. At these connection box the machine must be connected from the customer side (air supply, power supply, cables interface – Dietronic will provide a document for details).

**Motorized transport and locking for both machines**

The machine is equipped with a transportation mechanism on rails.

The wheelsets are guided by a guiding rail. With the help of a pole-changing braking gear motor the whole line can be moved into the line or out of the line.

There are two safety sensors at the entrance and at the exit that stop the machine inside or outside in the final position, the machine can be automatically fastened at the floor.

Motorized movement of the machines in and out of the line (SAFETY ENVIROMENTAL AREA MUST BE PROVIDED FROM THE BUYER)

The electrics and pneumatics connections pass along the machine side in a cable chain and can be plugged at both sides. A manufacturing drawing for the rails is included in our quotation. The supply and installation of the rails is not included in our scope of supply. In parking position, selected machine functions can be executed.

**Cable and Pipe Channels for both machines**

All channels to connect the connection boxes to the HMI and the connection boxes to the refilling units must be provided from a customer (Dietronic will provide a document for details) as well as the channel to connect the 2 connection boxes.

All cables and pipe from Dietronic side are scope of supply.

**Blank Transportation only for blank cleaner (stacker)**

Smart Conveyor ensures 100% of sheet movement without slitting by motorized removable pinch rolls transport conveyor and lifting pneumatic system for the IN and OUT of the dry-cleaner.

Upper round crushless wheels anti-slipping used for small parts gives correct movement of sheet metal, the solution to transfer short blank through the machine with min size W 400x L 400 mm.

**Electrical control**

The machine operating panel is placed separately according to the line layout.   
The control cabinets will be placed separately according to the line layout.

The control is equipped by Siemens.  
All the motors are SEW   
Armor Block Remote I/O Murr

**Software**

The software is provided in protected mode (only reading mode, not writing mode) until warranty expiration. The default language is English.

**Electrics & Control**

The communication is Profinet

The control cabinet can be placed on the structure of the machine.

The machine operating panel Siemens 9 inches HMI is placed separately according to the line.

The control is equipped by CPU 1517F and Point I/O and Safety I/O, which is placed in the control cabinet with air conditioning unit.


For the coil cleaner all the motors are SEW drive.

For the brush cleaner all the motors are Motovario

Armor Block Remote I/O Murr

Additional Mobile Panel for operating maintenance functions and displacement drive.

# **GENERAL DESCRIPTION COIL BRUSH CLEANER**

The linear brush wipes transversally across the product surface. Particles will cling to the micro-moistened filaments which will thus remove them effectively and transport them to the suction connection.

These results are possible thanks to:

- mechanical brush effect by the linear brush

-capillary adhesive forces between micro- moistened filament and particle

- reduction of electrostatic charges brought about by the DTBR\_300 (Ingromat) liquid.

**Linear Brushes**

Two Sword Brushes, wipe transversally across the material surfaces. The micro-moistened brush filaments (Antistatic Liquid system) remove even the most minute particles from the subject surface. The integrated pressure buffer provides for a constant wiping pressure and a premium cleaning result. The adjustment frame VE 25. allows a vertical adjustment of the Sword Brushes e.g. to adapt them to the material’s thickness or to remove them from the material surface for maintenance purposes.

Immagine che contiene stazionario

Descrizione generata automaticamenteTo protect the filaments and prolong the industrial life of the brushes, the linear brushes are lifted slightly at the edge of the strip and will touch the surface only after having just passed the material’s edge. The brushes at the inlet and outlet of the machine wipe in opposite directions, thus guaranteeing that the entire product surface is cleaned effectively.

**Pneumatic Height Adjustment**

The cleaning module may be mounted on an adjustment frame to integrate a height adjustment:

1. Manual adjustment via crank (HVM)
2. Electrical adjustment via actuator (HVE). An automatic thickness adjustment is possible if HVE is linked to the overall control
3. Pneumatic adjustment via pneumatic cylinder (HVP).

Quick removal of module from material surface, e.g. in crash situations. The mechanical and the electrical height adjustment may be combined with the pneumatic adjustment.

The brushes are supported by pneumatic pistons for fast opening.

A safety device before on the entrance of the machine is connected to the signal to open fast the brushes. The upper brush can be open for 200 mm and the lower for 100 mm.

**Self-Cleaning of the Brushes**

At the deviation, the linear brushes widen, so that particles may be detached more easily. Rotating steel elements (racks) remove the particles mechanically from the filaments. Additionally, there are com-pressed air driven nozzles, that blow into the brush filaments to cancel the capillary adhesive forces be-tween the particles and the filaments. The suction system will absorb the particles.

Benefit: Improved self-cleaning and automatic cleaning process

Steel and Dry alluminum:

only cyclone with heating

The patented Antistatic liquid system permits effective removal of even very fine particles.

**DTBR\_300 (Ingromat) Cleaning Liquid Applicator**

DTBR\_300 is an antistatic cleaning agent. The brush filaments are micro-moistened with DTBR\_300, thus providing an effective removal of even very fine dust particles

1. Micro-moistened brush filament with antistatic liquid
2. DTBR\_300 (Ingromat) sprayer SQL 51.
3. Distributor block VTB 100.
4. DTBR\_300 (Ingromat) regulator and filter unit IR 100. DTBR\_300 filter, dosage and display of inner pressure of pressure buffer
5. DTBR\_300 (INgromat) central supply pump, e.g. IS 102

The DTBR\_300 (Ingromat) liquid is supplied by a pneumatic from on frame tank of 20 lt tank with electric filling level control as well as pump and connections for refilling the reservoir.

Automatic refilling unit for the DTBR\_300 (Ingromat) tank from barrel or IBC Container 1000 lt.

The unit is provided with level sensor switch displayed on the HMI of the machine.

Calibrated nozzles control the amount of liquid applied on the single brush.

The consumption of the DTBR\_300 (Ingromat) is estimate in about 2L for hour.

|  |  |
| --- | --- |
| **BRUSHES SPECIFICATION** | |
| **NUMBER OF BRUSHES** | 8: 2 above, 2 below |
| **FILAMENTS** | black filaments in polyamide, length of filaments 17mm, diameter 0,2 mm |
| **SUCTION FILTER** | DUSTOMAT 4-10 |
| **BRUSH CLEANILESS LEVEL** | < 0,5 mm particle size |
| **DTBR\_300 (INGROMAT) RESERVOIR** | 50 litres |
| **UPPER BRUSH HEIGHT ADJUSTMENT** | automatic positioning of the upper brush |
| **SAFEY BRUSH DEVICE** | Will be supplied from Jier |

Immagine che contiene tavolo


Descrizione generata automaticamente

Cleaning performance 98% of particulars removal below 50 micro is required.

We can only confirm this requirement, when certain basic surface conditions are defined.

The cleaning results also can be influenced from initial conditions of the material.

# **GENERAL DESCRIPTION BLANKS BRUSH CLEANER**



The linear brush wipes transversally across the product surface. Particles will cling to the micro-moistened filaments which will thus remove them effectively and transport them to the suction connection.

These results are possible thanks to:

- mechanical brush effect by the linear brush

- capillary adhesive forces between micro- moistened filament and particle

- reduction of electrostatic charges brought about by the antistatic liquid.

**Linear Brushes**

Two Sword Brushes **(with 4 brushes belts for side)**, wipe transversally across the material surfaces. The micro-moistened brush filaments remove even the most minute particles from the subject surface. The integrated pressure buffer provides for a constant wiping pressure and a premium cleaning result. The adjustment frame VE 25. allows a vertical adjustment of the Sword Brushes e.g. to adapt them to the material’s thickness or to remove them from the material surface for maintenance purposes.

**Pneumatic Height Adjustment**

The cleaning module may be mounted on an adjustment frame to integrate a height adjustment:

1. Manual adjustment via crank (HVM)
2. Electrical adjustment via actuator (HVE). An automatic thickness adjustment is possible if HVE is linked to the overall control
3. Pneumatic adjustment via pneumatic cylinder (HVP).

Quick removal of module from material surface, e.g. in crash situations. The mechanical and the electrical height adjustment may be combined with the pneumatic adjustment.

The brushes are supported by pneumatic pistons for fast opening.

A safety device before on the entrance of the machine is connected to the signal to open fast the brushes. The upper brush can be open for 50 mm and the lower for 25 mm.

**Self-Cleaning of the Brushes**

At the deviation, the linear brushes widen, so that particles may be detached more easily. Rotating steel elements (racks) remove the particles mechanically from the filaments. Additionally, there are com-pressed air driven nozzles, that blow into the brush filaments to cancel the capillary adhesive forces be-tween the particles and the filaments. The suction system will absorb the particles.

Benefit: Improved self-cleaning and automatic cleaning process

Aluminum:

The cyclone has a level sensor to indicate when the tank is full suction duct is heated and monitored via temperature sensors

power supply and control

Steel:

Only cyclone without heating

The patented system permits effective removal of even very fine particles.

**DTBR Cleaner 300 (Ingromat), Cleaning Liquid Applicator**

The DTBR Cleaner 300 (Ingromat),is an antistatic cleaning agent. The brush filaments are micro-moistened with DTBR Cleaner 300, this providing an effective removal of even very fine dust particles

1. Micro-moistened brush filament with DTBR Cleaner 300 (Ingromat)
2. DTBR Cleaner 300 (Ingromat),sprayer SQL 51.
3. Distributor block VTB 100.
4. DTBR Cleaner 300 (Ingromat), regulator and filter unit IR 100. DTBR Cleaner 300 (Ingromat),filter, dosage and display of inner pressure of pressure buffer
5. DTBR Cleaner 300 (Ingromat),central supply pump, e.g. IS 102

The DTBR Cleaner 300 (Ingromat), liquid is supplied by a pneumatic from on frame tank of 20 lt tank with electric filling level control as well as pump and connections for refilling the reservoir.

Automatic refilling unit for the DTBR Cleaner 300 (Ingromat),tank from barrel or IBC Container 1000 lt.

The unit is provided with level sensor switch displayed on the HMI of the machine.

Calibrated nozzles control the amount of liquid applied on the single brush.

The consumption of the DTBR Cleaner 300 (Ingromat), is estimate in about 2L for hour.

**Extraction System Control**

The brushes are connected to an extraction system for the collection of the particular removed from the material.

An additional device “Cyclone” between the brushes and the extraction system allows the improvement of the filters life. In case of aluminum pre-coated with dry-lube, the recovery channels and the Cyclone are heated.

|  |  |
| --- | --- |
| **BRUSHES SPECIFICATION** | |
| **NUMBER OF BRUSHES** | 8: 4 above, 4 below |
| **FILAMENTS** | black filaments in polyamide, length of filaments 19mm, diameter 0,2 mm |
| **CYCLONE SYSTEM** | for pre-separation of oil removed (SZY 400) |
| **HEATING SYSTEM** | 60°C for all recovery channels |
| **SUCTION FILTER** | OEL-DS 1-0.28 |
| **BRUSH CLEANILESS LEVEL** | < 0,5 mm particle size |
| **ANTISTATIC LIQUID RESERVOIR** | 50 litres |
| **UPPER BRUSH HEIGHT ADJUSTMENT** | automatic positioning of the upper brush |
| **SAFEY BRUSH DEVICE** | laser sensor for anti-blank collision control for upper and lower brush (Dietronic will provide sensor and support, THE CUSTOMER will install on the infeed conveyor) |

Immagine che contiene tavolo

Descrizione generata automaticamente

According to the specification 98% of particulars removal below 50 micro is required.

We can only confirm this requirement, when certain basic surface conditions are defined.

The cleaning results also can be influenced from initial conditions of the material.

# **GENERAL SPECIFICATIONS INCLUDING IN THE QUOT****E**

|  |  |
| --- | --- |
| **Certification:** | QUASI MACHINE 2006/42/CE Machine Directive or CE Certification |
| **Labelling:** | DIETRONIC Standard |
| **Electrical schemes and drawings:** | PDF |
| **Notes:** | The software will be provided with comments only in English language. Until warranty expiration it will be provided only in readable version. Intellectual proprieties key-blocks of the program will be protected under password.  Colours of the machine:  -Body: RAL 9002  -Cabinet and operation panel: RAL 7035  -Rotating parts Covers: RAL 1003 |
| **Cables Standard Length** | Cable length 20 m |

|  |  |
| --- | --- |
| **Electrical BOM Part List** |  |
| PLC | Siemens 1517F |
| HMI | Two hand panel or Siemens HMI 7 inches |
| DC Power Supply | Cabur / Murr |
| Cabinet Carpentery | Rittal / DKC |
| Protection | Siemens / Murr |
| Plugs | Harting |
| Sensors | Ifm / Electrotech |
| Encoder | Leine Linde |
| Safety Relay | No |
| Frequency controller | Siemens G120 |
| Motor | SEW / Brushes (Motovario) |
| Armor block I/O | Murr |
| **Pneumatic BOM Part List** | SMC |

**Integration exclusion:**

-Downloading from truck

-Positioning on existing rail of the machine. DieTronic is not responsible about rails condition and alignment

-Re-assembling of parts dismounted for transportation (DieTronic supervision included)

-All the activities that require to fix on the concrete

Referred for sensor IN/OUT of the machine from the line

Cable chain

Connection box

-Communication devices and cable for software interface between our machine and the line including cable channels

-Software integration to the line

-Positioning of IBS or Barrel holder

-Channels and installation for flexible pipes to connect the Antistatic liquid from the IBC or Barrel holder to the connection box (flexible pipes included)

-Channels and installation for cables to connect the machine from connection box to the HMI pulpit (cables included)

-Installation and bracket of crash sensor

Cable for the sensor

Interface betwee the crash signal from the line to our machine

-Power supply and cable from the line to the connection box

-Piping for air supply from line to the connection box